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SPECIFICATION INSERT: SECTION 10 21 13
TOILET COMPARTMENT HARDWARE: HANDS-FREE STALL LOCK
Hy® Lock · SmartStall, Inc.
** NOTE TO SPECIFIER ** SmartStall, Inc.; hands-free restroom stall/cubicle locks. This section is based on the products of SmartStall, Inc., which is located at: Atlanta, GA, USA. Email: info@smartstallus.com. Web: https://www.smartstallus.com. SmartStall, Inc. manufactures the Hy® Lock, a hands-free, smart lock for restroom compartment doors that locks and unlocks with the wave of a hand and opens the door automatically for a no-touch exit. The Hy® Lock is designed to retrofit onto any partition system. How to use: For projects with new or replacement partitions, copy the paragraph below into the door hardware article of the toilet compartment section (10 21 13). Where existing partitions are to remain and the lock is the scope of work, use the complete Hy® Lock Guide Specification (CSI three-part format), available at www.smartstallus.com/guide-specification. Coordinate with Section 10 28 00 as applicable.
SPEC INSERT
** NOTE TO SPECIFIER ** Copy the single paragraph below into the door hardware article of Section 10 21 13, renumbering to match the sequence of the edited section. Retain one bracketed finish and delete the other. Distributors may reproduce this paragraph verbatim in project specification packages.
A. Hands-Free Stall Latch: Hy® Lock 
Manufactured by SmartStall, Inc., Atlanta, GA; Website: www.smartstallus.com. 
1. Operation: Hands-free lock and unlock via wave sensor with full manual operation via mechanical knob at all times, including power loss; the door swings open automatically upon unlock for inswing-oriented doors utilizing gravity hinges. 
2. Power Source: Battery-powered. 
3. Occupancy Indicator: Lock-state indication visible from interior and exterior of compartment; emergency release operable from exterior of compartment. 
4. Finish: [Satin Aluminum] [Matte Black]. 
5. Coordination: Provide gravity-type or similar self-closing/opening hinges; coordinate with partition hinge selection. Locate combination door stop and coat hook accessories on the panel, pilaster, or wall toward which the door closes; do not mount on the compartment door. 
6. Accessibility: Manual operation complying with 2010 ADA Standards and ICC A117.1 operable with one hand, without tight grasping, pinching, or twisting of the wrist.
7. Keepers: Suitable for inswing and outswing doors; provide keeper type corresponding to door swing as indicated on Drawings.
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